Operation: | Update Central Management
Description: | Manage and monitor the appliance through Central Management.

Sample Configuration
    	<CentralManagement>
    		<ManageUsingCentralManagement>Enable/Disable</ManageUsingCentralManagement>
    		<ServerAddress>ip</ServerAddress>
    		<ApplianceManagement>
    			<ConfigurationManagement>Enable/Disable</ConfigurationManagement>
    			<CommunicationDetails>
    				<HeartbeatProtocol>Syslog/HTTPS</HeartbeatProtocol>
    				<HeartbeatPort>514</HeartbeatPort>
    			</CommunicationDetails>
    			<ConfigurationSyncronization>
    				<Mode>Push/Pull</Mode>
    				<Port>443</Port>
    			</ConfigurationSyncronization>
    		</ApplianceManagement>
    		<SignatureUpdates>
    			<SignatureDistribution>Enable/Disable</SignatureDistribution>
    			<Port>80</Port>
    		</SignatureUpdates>
    	</CentralManagement>

Attribute/Parameter Information :

Parameter | Mandatory | Default | Description
--- | --- | --- | ---
ManageUsingCentralManagement | No |  | Description: Enable to manage the appliance through Central Management. ManageUsingCentralManagement confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only 'yes', 'YES' are allowed.
ServerAddress | No |  | Description: Specify the IPv4 address/domain for Central Management. ServerAddress confines to: Type is 'SCALAR'. Datatype is 'IPADDRESS','DOMAIN','IPADDRESS6'. Maximum characters allowed are 255. IP Class other than 'MULTICAST', 'RESERVED', 'LOCALHOST', 'UNSPECIFIED', 'BROADCAST', 'LINKLOCAL' is allowed.
HeartbeatProtocol | No |  | Description: Select Heartbeat protocol from the options available. It specifies how the information will be provided to Central Management. HeartbeatProtocol confines to: Type is 'SCALAR'. Datatype is 'STRING'.
HeartbeatPort | No | 80 | Description: Specify the Heartbeat port. This is the port used for Keep Alive requests used by Central Management to check if Appliance is up. HeartbeatPort confines to: Type is 'SCALAR'. Datatype is 'INTEGER'. Allowed numbers: 1 to 65535. Maximum digits allowed are 5.
Mode | No |  | Description: Select the mode for sending configuration updates. Mode confines to: Type is 'SCALAR'. Datatype is 'STRING'.
Protocol | No |  | Description: Select connection protocol for sending updates. Protocol confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only 'https', 'http' are allowed.
Port | No |  | Description: Specify the port number of the selected connection protocol. Port confines to: Type is 'SCALAR'. Datatype is 'INTEGER'. Allowed numbers: 1 to 65535. Maximum digits allowed are 5.
Port | Yes |  | Description: If Central Management is selected for receiving Signature Updates, Specify Central Management Port. Port confines to: Type is 'SCALAR'. Datatype is 'INTEGER'. Allowed numbers: 1 to 65535. Maximum digits allowed are 5.
SecureCommunication | No | Disable | Description: Enable to ensure secure communication between Appliance and Central Management. SecureCommunication confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only 'true', 'false' are allowed.

Status Message Information :

Operation | Status | Message
--- | --- | ---
Update Central Management | 200 |
Update Central Management | 500 |

) Copyright 2015 Sophos Limited. All rights reserved.
Sophos is registered trademarks of Sophos Limited and Sophos Group. All other product and company names mentioned are trademarks or registered trademarks of their respective owners.No part of this publication may be reproduced, stored in a retrieval system, or transmitted, in any form or by any means, electronic, mechanical, photocopying, recording or otherwise unless you are either a valid licensee where the documentation can be reproduced in accordance with the license terms or you otherwise have the prior permission in writing of the copyright owner.