Operation: | Add Policy Route / Update Policy Route
Description: | Add a Policy RouteUpdate a Policy Route

Sample Configuration
    	<PolicyRoute>
    		<Name>Default</Name>
    		<Description />
    		<IPFamily>{0/1}</IPFamily><!-- default IPv4 -->
    		<Gateway>ip</Gateway>
    		<Interface>{interface}</Interface>
    		<DSCPMarking>0-Best Effort/1/2/3/4/5/6/7/8-Class 1(CS1)/9/10-Class 1,Gold(AF11)/11/12-Class1,Silver(AF12)/13/14-Class 1,Bronze(AF13)/15/16-Class 2(CS2)/17/18-Class 2,Gold(AF21)/19/20-Class 2,Silver(AF22)/21/22-Class 2,Bronze(AF23)/23/24-Class 3(CS3)/25/26-Class 3,Gold(AF31)/27/28-Class 3,Silver(AF32)/29/30-Class 3,Bronze(AF33)/31/32-Class 4(CS4)/33/34-Class 4,Gold(AF41)/35/36-Class 4,Silver(AF42)/37/38-Class 4,Bronze(AF43)/39/40-Class 5(CS5)/41/42/43/44/45/46-Expedited Forwarding(EF)/47/48-Control(CS6)/49/50/51/52/53/54/55/56-Control(CS7)/57/58/59/60/61/62/63</DSCPMarking>
    		<SourceNetworks>
    			<Network>Source Network</Network>
    			<Network>Source Network</Network>
    			:
    		</SourceNetworks>
    		<Services>
    			<Service>servicename</Service>
    			:
    		</Services>
    		<DestinationNetworks>
    			<Network>Destinaiton Network</Network>
    			<Network>Destinaiton Network</Network>
    			:
    		</DestinationNetworks>
    	</PolicyRoute>

Attribute/Parameter Information :

Parameter | Mandatory | Default | Description
--- | --- | --- | ---
Name | Yes |  | Description: Specify a name for policy route. Name confines to: Type is 'SCALAR'. Datatype is 'STRING'. Comma (,) is not allowed. Maximum characters allowed are 60. UTF-8 character(s) are allowed.
Description | No |  | Description: Specify a description for Policy Route. Description confines to: Type is 'SCALAR'. Datatype is 'STRING'. Maximum characters allowed are 255.
IPFamily | Yes | IPv4 | Description: Select the IP family. IPFamily confines to: Type is 'SCALAR'. Datatype is 'INTEGER'. Only '0', '1' are allowed.
SourceNetworks | No |  | Description: Select the source network(s) of the packet to be routed. SourceNetworks confines to: Type is 'ARRAY'. Datatype is 'STRING'. Maximum characters allowed are 60. Multiple values are allowed.
DestinationNetworks | No |  | Description: Select the destination network(s) of the packet to be routed. DestinationNetworks confines to: Type is 'ARRAY'. Datatype is 'STRING'. Maximum characters allowed are 60. Multiple values are allowed.
Services | No |  | Description: Select the services(s) of the packet to be routed. Services confines to: Type is 'ARRAY'. Datatype is 'STRING'. Maximum characters allowed are 60. Multiple values are allowed.
DSCPMarking | No |  | Description: Select the type of DSCP Marking to match the packets marked with the given DSCP value. DSCPMarking confines to: Type is 'SCALAR'. Datatype is 'STRING'.
Gateway | Yes |  | Description: Select the gateway to which you want to forward the packet if the packet meets the configured matching criteria. Gateway confines to: Type is 'SCALAR'. Datatype is 'STRING'.
Interface | No |  | Description: Select the incoming interface receiving the packet. Interface confines to: Type is 'SCALAR'. Datatype is 'STRING'.

Status Message Information :

Operation | Status | Message
--- | --- | ---
Update Policy Route | 200 |
Update Policy Route | 500 |
Add Policy Route | 200 |
Add Policy Route | 500 |
Add Policy Route | 502 |

) Copyright 2015 Sophos Limited. All rights reserved.
Sophos is registered trademarks of Sophos Limited and Sophos Group. All other product and company names mentioned are trademarks or registered trademarks of their respective owners.No part of this publication may be reproduced, stored in a retrieval system, or transmitted, in any form or by any means, electronic, mechanical, photocopying, recording or otherwise unless you are either a valid licensee where the documentation can be reproduced in accordance with the license terms or you otherwise have the prior permission in writing of the copyright owner.