Operation: | HA Configuration-HA Settings
Description: | Configure High Availability. It is a feature wherein two appliances are grouped together in a cluster and instructed to work as a single entity.

Sample Configuration
    	<HA>
    		<HAConfigure>
    			<!--ApplianceKey is readonly purpose -->
    			<HAConfiguration>EnableHA</HAConfiguration>
    			<!-- IF HAConfiguration is EnableHA then all below options are required. -->
    			<ApplianceKey>C017204597-AB5DQ6</ApplianceKey>
    			<PeerApplianceKey>C017204597-AB5DQ6</PeerApplianceKey>
    			<HAConfigurationMode>Active-Active/Active-Passive</HAConfigurationMode>
    			<DedicatedHALinkPort>PortC</DedicatedHALinkPort>
    			<PeerHALinkIP>1.1.1.1</PeerHALinkIP>
    			<PeerAdministrationPort>PortA</PeerAdministrationPort>
    			<PeerAdministrationIP>1.1.1.1</PeerAdministrationIP>
    			<PeerAdministrationIPV6>1122::1211</PeerAdministrationIPV6>
    			<MonitoredPorts>
    				<Port>Number</Port>
    				:
    			</MonitoredPorts>
    		</HAConfigure>
    		<DisableHA>actionidentificationtagnodata</DisableHA> <!-- this tag is just a event indication -->
    	</HA>

Attribute/Parameter Information :

Parameter | Mandatory | Default | Description
--- | --- | --- | ---
HAConfigurationMode | Yes |  | Description: Select configuration mode for the cluster from the available options: Active-Active OR Active-Passive. HAConfigurationMode confines to: Type is 'SCALAR'. Datatype is 'STRING'.
Port | No |  | Description: Select the port for Heartbeat Link using which both Appliances in HA would monitor each other. Port confines to: Type is 'SCALAR'. Datatype is 'STRING'.
PeerAdministrationIP | Yes |  | Description: Specify Administration IP Address for Auxiliary Appliance using which the Admin Console of Auxiliary Appliance can be accessed. PeerAdministrationIP confines to: Type is 'SCALAR'. Datatype is 'IPADDRESS'. Maximum characters allowed are 30. IP Class other than 'MULTICAST', 'RESERVED', 'LOCALHOST', 'UNSPECIFIED', 'BROADCAST', 'LINKLOCAL' is allowed.
PeerAdministrationPort | Yes |  | Description: Specify Administration Port for Auxiliary Appliance. PeerAdministrationPort confines to: Type is 'SCALAR'. Datatype is 'STRING'.
Port | No |  | Description: Select the ports to be monitored and in case any port goes down, the appliance will leave cluster. Port confines to: Type is 'SCALAR'. Datatype is 'STRING'.
DedicatedHALinkPort | Yes |  | Description: Specify HA link port through which the two appliances are physically connected. DedicatedHALinkPort confines to: Type is 'SCALAR'. Datatype is 'STRING'.
PeerHALinkIP | Yes |  | Description: Specify IP Address configured on the HA link port of the peer appliance. PeerHALinkIP confines to: Type is 'SCALAR'. Datatype is 'IPADDRESS'. Maximum characters allowed are 30. IP Class other than 'MULTICAST', 'RESERVED', 'LOCALHOST', 'UNSPECIFIED', 'BROADCAST', 'LINKLOCAL' is allowed.
EncryptionKey | Yes |  | Description: Specify 'encryptionkey' EncryptionKey confines to: Type is 'SCALAR'. Datatype is 'STRING'. Maximum characters allowed are 16. Minimum characters allowed are 8.
PeerAdministrationIPV6 | No |  | Description: Specify 'peeraccessipv6' PeerAdministrationIPV6 confines to: Type is 'SCALAR'. Datatype is 'STRING'.

Status Message Information :

Operation | Status | Message
--- | --- | ---
HA Configuration-HA Settings | 200 |
HA Configuration-HA Settings | 211 |
HA Configuration-HA Settings | 216 |
HA Configuration-HA Settings | 500 |
HA Configuration-HA Settings | 502 |
HA Configuration-HA Settings | 504 |
HA Configuration-HA Settings | 505 |
HA Configuration-HA Settings | 541 |
HA Configuration-HA Settings | 542 |
HA Configuration-HA Settings | 543 |
HA Configuration-HA Settings | 544 |
HA Configuration-HA Settings | 545 |
HA Configuration-HA Settings | 546 |
HA Configuration-HA Settings | 547 |
HA Configuration-HA Settings | 548 |
HA Configuration-HA Settings | 549 |
HA Configuration-HA Settings | 550 |
HA Configuration-HA Settings | 551 |

) Copyright 2015 Sophos Limited. All rights reserved.
Sophos is registered trademarks of Sophos Limited and Sophos Group. All other product and company names mentioned are trademarks or registered trademarks of their respective owners.No part of this publication may be reproduced, stored in a retrieval system, or transmitted, in any form or by any means, electronic, mechanical, photocopying, recording or otherwise unless you are either a valid licensee where the documentation can be reproduced in accordance with the license terms or you otherwise have the prior permission in writing of the copyright owner.