Operation: | Add IPv6 DHCP Server / Edit IPv6 DHCP Server
Description: | This json is used to add IPv6 DHCP ServerThis json is used to update IPv6 DHCP Server

Sample Configuration
    	<DHCPServerIpv6>
    	<Name>Name</Name>
    	<Interface>PortA</Interface>
    	<IPLease>
    			<IP>StartIPAddress-EndIPAddress</IP>
    			:
    	</IPLease>
    	<StaticLease>
    			<Lease>
    				<HostName>host</HostName>
    				<DUID>duid</DUID>
    				<IPAddress>ip</IPAddress>
    			</Lease>
    			:
    	</StaticLease>
    	<UseApplianceDNSSettings>Enable</UseApplianceDNSSettings>
    	<PreferredTime>540</PreferredTime>
    	<ValidTime>720</ValidTime>
    	<PrimaryDNSServer>DNSIPAddress</PrimaryDNSServer>
    	<SecondaryDNSServer>DNSIPAddress</SecondaryDNSServer>
    	</DHCPServerIpv6>

Attribute/Parameter Information :

Parameter | Mandatory | Default | Description
--- | --- | --- | ---
Name | Yes |  | Description: Specify name for DHCP Server. Name confines to: Type is 'SCALAR'. Datatype is 'STRING'. Comma (,) is not allowed. Maximum characters allowed are 50. UTF-8 character(s) are allowed.
Interface | No |  | Description: Select interface on which DHCP Service is to be configured. Interface confines to: Type is 'SCALAR'. Datatype is 'STRING'.
Host Name | No |  | Description: Specify host name if lease type selected is 'Static' where specific IP addresses are assigned to the clients. Host Name confines to: Type is 'ARRAY'. Datatype is 'STRING'. Maximum characters allowed are 50. Multiple values are allowed.
DUID | No |  | Description: Specify 'duid' DUID confines to: Type is 'ARRAY'. Datatype is 'STRING'. Maximum characters allowed are 72. Multiple values are allowed.
IP Address | No |  | Description: Specify IP Address for MAC-IP mapping for 'Static' lease type. IP Address confines to: Type is 'ARRAY'. Datatype is 'IPADDRESS6'. Maximum characters allowed are 51. Multiple values are allowed. Duplicate values will not be ignored. IP Class other than 'MULTICAST', 'LOCALHOST', 'UNSPECIFIED', 'LINKLOCAL' is allowed.
preferredtime | Yes |  | Description: Specify preferred time. preferredtime confines to: Type is 'SCALAR'. Datatype is 'INTEGER'. Range 1 to 43200 is allowed. Maximum digits allowed are 5.
validtime | Yes |  | Description: Specify valid time. validtime confines to: Type is 'SCALAR'. Datatype is 'INTEGER'. Range 1 to 43200 is allowed. Maximum digits allowed are 5.
Use Appliance's DNS Settings | No |  | Description: Specify Enable/Disable for Appliance's DNS Settings Use Appliance's DNS Settings confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only 'on' are allowed.
primarydnsv6 | No |  | Description: Provide Primary DNS Server IP Address if appliance DNS Server is not to be used. primarydnsv6 confines to: Type is 'SCALAR'. Datatype is 'IPADDRESS6'. Maximum characters allowed are 51. IP Class other than 'MULTICAST', 'UNSPECIFIED', 'LINKLOCAL' is allowed.
secondarydnsv6 | No |  | Description: Provide Secondary DNS Server IP Address if appliance DNS Server is not be used. secondarydnsv6 confines to: Type is 'SCALAR'. Datatype is 'IPADDRESS6'. Maximum characters allowed are 51. IP Class other than 'MULTICAST', 'UNSPECIFIED', 'LINKLOCAL' is allowed.
Lease IP Range | No |  | Description: Specify IP Address range from which DHCP Server will assign addresses to the clients. Lease IP Range confines to: Type is 'ARRAY'. Datatype is 'STRING'. Maximum characters allowed are 105. Multiple values are allowed. Duplicate values will not be ignored. IP Class other than 'MULTICAST', 'LOCALHOST', 'UNSPECIFIED', 'LINKLOCAL' is allowed.

Status Message Information :

Operation | Status | Message
--- | --- | ---
Edit IPv6 DHCP Server | 200 |
Edit IPv6 DHCP Server | 500 |
Edit IPv6 DHCP Server | 541 |
Edit IPv6 DHCP Server | 542 |
Edit IPv6 DHCP Server | 543 |
Edit IPv6 DHCP Server | 544 |
Edit IPv6 DHCP Server | 545 |
Edit IPv6 DHCP Server | 547 |
Add IPv6 DHCP Server | 200 |
Add IPv6 DHCP Server | 500 |
Add IPv6 DHCP Server | 502 |
Add IPv6 DHCP Server | 542 |
Add IPv6 DHCP Server | 541 |
Add IPv6 DHCP Server | 543 |
Add IPv6 DHCP Server | 545 |
Add IPv6 DHCP Server | 544 |
Add IPv6 DHCP Server | 547 |

) Copyright 2015 Sophos Limited. All rights reserved.
Sophos is registered trademarks of Sophos Limited and Sophos Group. All other product and company names mentioned are trademarks or registered trademarks of their respective owners.No part of this publication may be reproduced, stored in a retrieval system, or transmitted, in any form or by any means, electronic, mechanical, photocopying, recording or otherwise unless you are either a valid licensee where the documentation can be reproduced in accordance with the license terms or you otherwise have the prior permission in writing of the copyright owner.