Operation: | Add IP Tunnel / Edit IP Tunnel
Description: | To Add/Edit IP Tunnel. IP Tunnel is an Internet Protocol network communications path between two networks.

Sample Configuration
    	<IPTunnel>
    		<Name>Name</Name>
    		<TunnelType>6in4/6to4/6rd/4in6</TunnelType>
    		<Zone>zonename</Zone>
    		<LocalEndPoint>ipaddress</LocalEndPoint>
    		<RemoteEndPoint>ipaddress</RemoteEndPoint>
    		<TTL>Number</TTL>
    		<TOS>Number</TOS>
    		<Prefix>Text</Prefix>
    	</IPTunnel>

Attribute/Parameter Information :

Parameter | Mandatory | Default | Description
--- | --- | --- | ---
Name | No |  | Description: Specify a name for the tunnel. Name confines to: Type is 'SCALAR'. Datatype is 'STRING'. First character is to be alphabet (a-zA-Z). Alphanumeric (a-zA-Z0-9) and underscore (_) to be allowed for the remaining characters. Maximum characters allowed are 10.
TunnelType | Yes |  | Description: Select the type of tunnel from the available options: 6in4, 6to4, 6rd or 4in6. TunnelType confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only '15', '16', '17', '18' are allowed.
Zone | Yes |  | Description: Select the Zone from the available options: LAN, WAN or DMZ. Zone confines to: Type is 'SCALAR'. Datatype is 'STRING'.
LocalEndPoint | Yes |  | Description: Specify IP Address of the Local End Point of the tunnel. LocalEndPoint confines to: Type is 'SCALAR'. Datatype is 'IPADDRESS'. IP Class other than 'MULTICAST', 'RESERVED', 'LOCALHOST', 'UNSPECIFIED', 'BROADCAST', 'LINKLOCAL' is allowed.
RemoteEndPoint | Yes |  | Description: Specify IP Address of the Remote End Point of the tunnel. RemoteEndPoint confines to: Type is 'SCALAR'. Datatype is 'IPADDRESS'. IP Class other than 'MULTICAST', 'RESERVED', 'LOCALHOST', 'UNSPECIFIED', 'BROADCAST', 'LINKLOCAL' is allowed.
TTL | No | 0 | Description: Specify the life time of data. TTL confines to: Type is 'SCALAR'. Datatype is 'INTEGER'. Range 0 to 255 is allowed.
TOS | No | 0 | Description: Specify the priority of data. TOS confines to: Type is 'SCALAR'. Datatype is 'INTEGER'. Range 0 to 99 is allowed.
Prefix | No |  | Description: Specify Prefix if selected tunnel type is '6rd'. Prefix confines to: Type is 'SCALAR'. Datatype is 'STRING'.

Status Message Information :

Operation | Status | Message
--- | --- | ---
Edit IP Tunnel | 200 |
Edit IP Tunnel | 500 |
Edit IP Tunnel | 503 |
Add IP Tunnel | 200 |
Add IP Tunnel | 500 |
Add IP Tunnel | 502 |
Add IP Tunnel | 503 |

) Copyright 2015 Sophos Limited. All rights reserved.
Sophos is registered trademarks of Sophos Limited and Sophos Group. All other product and company names mentioned are trademarks or registered trademarks of their respective owners.No part of this publication may be reproduced, stored in a retrieval system, or transmitted, in any form or by any means, electronic, mechanical, photocopying, recording or otherwise unless you are either a valid licensee where the documentation can be reproduced in accordance with the license terms or you otherwise have the prior permission in writing of the copyright owner.