Operation: | Add Trusted MAC / Update Trusted MAC
Description: | To Create/Update Trusted MAC list which filters the devices that can access network.

Sample Configuration
    	<TrustedMAC>
    		<!-- Either manual addition or using file import -->
    		<MACAddress>macaddress</MACAddress>
    		<AssociateIP>ip address</AssociateIP>
    		<IPV4Association>None/Static/DHCP</IPV4Association>
    		<IPV4Address>IPAddress</IPV4Address>
    		<IPV6Association>None/Static/DHCP</IPV6Association>
    		<IPV6Address>IPAddress</IPV6Address>
    		<OldConfiguration>
    			<MACAddress>macaddress</MACAddress>
    		</OldConfiguration>
    	</TrustedMAC>

Attribute/Parameter Information :

Parameter | Mandatory | Default | Description
--- | --- | --- | ---
MACAddress | Yes |  | Description: Specify MAC Address to be added to the Trusted MAC List. MACAddress confines to: Type is 'SCALAR'. Datatype is 'MACADDRESS'. Maximum characters allowed are 17.
IPV4Association | No | Static | Description: Select IP Association type for binding IPv4 Address to MAC Address. IPV4Association confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only '1', '2', '0' are allowed.
IPV4Address | No |  | Description: Specify IPv4 Address for IP-MAC binding. IPV4Address confines to: Type is 'CSV'. Datatype is 'IPADDRESS'. Comma separated values are allowed. Maximum characters allowed are 15. IP Class other than 'MULTICAST', 'RESERVED', 'LOCALHOST', 'UNSPECIFIED', 'BROADCAST', 'LINKLOCAL' is allowed.
IPV6Address | No |  | Description: Specify IPv6 Address for IP-MAC binding. IPV6Address confines to: Type is 'CSV'. Datatype is 'IPADDRESS6'. Comma separated values are allowed. Maximum characters allowed are 39. IP Class other than 'MULTICAST', 'LOCALHOST', 'UNSPECIFIED' is allowed.
AssociateIP | No |  | Description: Enable/Disable IP Association. AssociateIP confines to: Type is 'SCALAR'. Datatype is 'STRING'.
IPV6Association | No | Static | Description: Select IP Association type for binding IPv6 Address to MAC Address. IPV6Association confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only '1', '2', '0' are allowed.

Status Message Information :

Operation | Status | Message
--- | --- | ---
Update Trusted MAC | 200 | Operation Successful.
| Update Trusted MAC | 500 | Operation Fail. Add Trusted MAC | 200 | Operation Successful.
| Add Trusted MAC | 500 | Operation Fail.

) Copyright 2017 Sophos Limited. All rights reserved.
Sophos is registered trademarks of Sophos Limited and Sophos Group. All other product and company names mentioned are trademarks or registered trademarks of their respective owners.No part of this publication may be reproduced, stored in a retrieval system, or transmitted, in any form or by any means, electronic, mechanical, photocopying, recording or otherwise unless you are either a valid licensee where the documentation can be reproduced in accordance with the license terms or you otherwise have the prior permission in writing of the copyright owner.