Operation: | Add Zone / Edit Zone / Edit Zone from API
Description: | To Add/Edit Zone. Zone is a logical grouping of physical interfaces/ports.

Sample Configuration
    	<Zone>
    		<Name>zonename</Name>
    		<Type>LAN/DMZ</Type>
    		<!-- MemberPorts are for readonly purpose -->
    		<Description>Text</Description>
    		<ApplianceAccess>
    			<AdminServices>
    				<HTTP>Enable/Disable</HTTP>
    				<HTTPS>Enable/Disable</HTTPS>
    				<Telnet>Enable/Disable</Telnet>
    				<SSH>Enable/Disable</SSH>
    			</AdminServices>
    			<AuthenticationServices>
    				<Windows-LinuxClient>Enable/Disable</Windows-LinuxClient>
    				<CaptivePortal>Enable/Disable</CaptivePortal>
    				<NTLM>Enable/Disable</NTLM>
    				<RadiusSSO>Enable/Disable</RadiusSSO>
    			</AuthenticationServices>
    			<NetworkServices>
    				<DNS>Enable/Disable</DNS>
    				<Ping>Enable/Disable</Ping>
    			</NetworkServices>
    			<OtherServices>
    				<WebProxy>Enable/Disable</WebProxy>
    				<SSLVPN>Enable/Disable</SSLVPN>
    			</OtherServices>
    		</ApplianceAccess>
    	</Zone>

Attribute/Parameter Information :

Parameter | Mandatory | Default | Description
--- | --- | --- | ---
Name | Yes |  | Description: Specify a name to identify the Zone. Name confines to: Type is 'SCALAR'. Datatype is 'STRING'. First character is to be Alphanumeric except ZERO '0' (1-9a-zA-Z). Alphanumeric (a-zA-Z0-9) and underscore (_) to be allowed for the remaining characters. Maximum characters allowed are 60.
Type | Yes | LAN | Description: Select the type of Zone from the available options: LAN or DMZ. Type confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only '1', '2', '3', '4', '5', '6' are allowed.
MemberPorts | No |  | Description: Displays all the member ports of the particular Zone selected. MemberPorts confines to: Type is 'CSV'. Datatype is 'STRING'. Comma separated values are allowed.
Description | No |  | Description: Specify Zone description. Description confines to: Type is 'SCALAR'. Datatype is 'STRING'. Maximum characters allowed are 60.
SSH/NTLM/Windows-LinuxClient/HTTP/WebProxy/Telnet/CaptivePortal/DNS/SSLVPN/Ping/RadiusSSO/HTTPS | No |  | Description: Define the type of administrative access permitted on zone. SSH/NTLM/Windows-LinuxClient/HTTP/WebProxy/Telnet/CaptivePortal/DNS/SSLVPN/Ping/RadiusSSO/HTTPS confines to: Type is 'ARRAY'. Datatype is 'STRING'. Only '1', '2', '3', '4', '5', '6', '7', '8', '9', '10', '11', '12', '13', '14', '18', '23', '38', '39', '40' are allowed. Multiple values are allowed.

Status Message Information :

Operation | Status | Message
--- | --- | ---
Edit Zone | 200 |
Edit Zone | 500 |
Edit Zone from API | 200 |
Edit Zone from API | 500 |
Add Zone | 200 |
Add Zone | 500 |
Add Zone | 502 |
Add Zone | 510 |

) Copyright 2017 Sophos Limited. All rights reserved.
Sophos is registered trademarks of Sophos Limited and Sophos Group. All other product and company names mentioned are trademarks or registered trademarks of their respective owners.No part of this publication may be reproduced, stored in a retrieval system, or transmitted, in any form or by any means, electronic, mechanical, photocopying, recording or otherwise unless you are either a valid licensee where the documentation can be reproduced in accordance with the license terms or you otherwise have the prior permission in writing of the copyright owner.