Operation: | Add LAG / Edit LAG
Description: | To Add/Edit Link Aggregation Group(LAG)interfaces. LAG interfaces allows multiple physical links to be combined into a single logical link.

Sample Configuration
    	<LAG>
    		<Name>interfacename</Name>
    		<MemberInterface>
    			<Interface>interfacename</Interface>
    			:
    		</MemberInterface>
    		<Mode>ActiveBackup/802.3ad(LACP)</Mode>
    		<NetworkZone>zonename</NetworkZone>
    		<IPAssignment>Static/DHCP</IPAssignment>
    		<!-- IPv4Configuration -->
    		<IPv4Configuration>Enable/Disable</IPv4Configuration>
    		<IPAssignment>Static/PPPoe/DHCP</IPAssignment>
    		<IPv4Address>ipaddress</IPv4Address>
    		<Netmask>netmask</Netmask>
    		<GatewayName>Text</GatewayName>
    		<GatewayIP>ip address</GatewayIP>

    		<!-- IPv6Configuration -->
    		<IPv6Configuration>Enable/Disable</IPv6Configuration>
    		<IPv6Address>ipaddress</IPv6Address>
    		<Prefix>Number</Prefix>
    		<GatewayNameIpv6>Text</GatewayNameIpv6>
    		<GatewayIPv6>ipv6 address</GatewayIPv6>
    		<InterfaceSpeed>Auto Negotiate/10MbpsHD/10MbpsFD/100MbpsHD/100MbpsFD/1000MbpsFD/1000MbpsHD/10000MbpsFD</InterfaceSpeed>
    		<MTU>Number</MTU>
    		<MSS>
    			<OverrideMSS>Enable/Disable</OverrideMSS>
    			<MSSValue>Number</MSSValue>
    		</MSS>
    		<XmitHashPolicy>Layer2/Layer2+3/Layer3+4</XmitHashPolicy>
    		<MACAddress>Default/{userdefined MAC Address}</MACAddress>
    	</LAG>

Attribute/Parameter Information :

Parameter | Mandatory | Default | Description
--- | --- | --- | ---
Name/LagInterface | Yes |  | Description: Specify the name for LAG interface. Name/LagInterface confines to: Type is 'SCALAR'. Datatype is 'STRING'. Comma (,) is not allowed. Maximum characters allowed are 10. UTF-8 character(s) are allowed.
Interface | Yes |  | Description: Select the ports from the list which are the members of the interface. Interface confines to: Type is 'ARRAY'. Datatype is 'STRING'. Multiple values are allowed.
Mode | Yes |  | Description: Select the mode of LAG from available options: Active-Passive and 802.3ad (LACP). Mode confines to: Type is 'SCALAR'. Datatype is 'STRING'.
NetworkZone | Yes |  | Description: Select Network zone for the interface. NetworkZone confines to: Type is 'SCALAR'. Datatype is 'STRING'.
IPAssignment | Yes | Static | Description: Select the IP Assignment Scheme from the available options. IPAssignment confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only '0', '2' are allowed.
IPv4Address | No |  | Description: Specify IPv4 address for the interface. IPv4Address confines to: Type is 'SCALAR'. Datatype is 'IPADDRESS'. Maximum characters allowed are 15. IP Class other than 'MULTICAST', 'RESERVED', 'LOCALHOST', 'UNSPECIFIED', 'BROADCAST', 'NETWORKBROADCAST', 'NETWORKIP' is allowed.
Netmask | No |  | Description: Specify Network Subnet mask for the interface. Netmask confines to: Type is 'SCALAR'. Datatype is 'IPADDRESS'. Maximum characters allowed are 15.
GatewayName | No |  | Description: Specify Gateway name through which traffic is to be routed. GatewayName confines to: Type is 'SCALAR'. Datatype is 'STRING'. Maximum characters allowed are 50.
GatewayIP | No |  | Description: Specify Gateway IPv4 Address. GatewayIP confines to: Type is 'SCALAR'. Datatype is 'IPADDRESS'. Maximum characters allowed are 15.
InterfaceSpeed | No |  | Description: Select Interface speed for Synchronization. InterfaceSpeed confines to: Type is 'SCALAR'. Datatype is 'STRING'.
MTU | Yes | 1500 | Description: Specify Maximum Transmission Unit(MTU)value. MTU confines to: Type is 'SCALAR'. Datatype is 'INTEGER'. Range 576 to 1500 is allowed. Maximum digits allowed are 4.
MSSValue | Yes | Enable | Description: Select to specify Maximum Segment Size(MSS)to override default MSS. MSSValue confines to: Type is 'SCALAR'. Datatype is 'INTEGER'. Range 536 to 1460 is allowed. Maximum digits allowed are 4.
XmitHashPolicy | Yes |  | Description: Select the Xmit hash Policy to be used for member interfaces from the options available: Layer2, Layer2+3, Layer 3+4. XmitHashPolicy confines to: Type is 'SCALAR'. Datatype is 'STRING'. Note: Available only if 802.3ad LACP mode is selected.
MACAddress | Yes | Enable | Description: Select to use default MAC Address. MACAddress confines to: Type is 'SCALAR'. Datatype is 'MACADDRESS'. Maximum characters allowed are 17.
GatewayNameIpv6 | No |  | Description: Used to configure Gateway Name for IPv6 Configuration. GatewayNameIpv6 confines to: Type is 'SCALAR'. Datatype is 'STRING'. Maximum characters allowed are 50.
GatewayIPv6 | No |  | Description: Used to set IPv6 address for Gateway in IPv6 Configuration. GatewayIPv6 confines to: Type is 'SCALAR'. Datatype is 'STRING'. Maximum characters allowed are 45.
IPv6Address | No |  | Description: Used to set IPv6 address for interface in IPv6 Configuration. IPv6Address confines to: Type is 'SCALAR'. Datatype is 'IPADDRESS6'. Maximum characters allowed are 45. IP Class other than 'MULTICAST', 'LOCALHOST', 'UNSPECIFIED', 'BROADCAST', 'LINKLOCAL', 'NETWORKBROADCAST', 'NETWORKIP' is allowed.
Prefix | No |  | Description: Used to set Prefix for Physical interface in IPv6 Configuration. Prefix confines to: Type is 'SCALAR'. Datatype is 'INTEGER'. Range 1 to 128 is allowed. Maximum digits allowed are 3.

Status Message Information :

Operation | Status | Message
--- | --- | ---
Edit LAG | 200 |
Edit LAG | 500 |
Edit LAG | 502 |
Edit LAG | 503 |
Edit LAG | 507 |
Edit LAG | 541 |
Edit LAG | 542 |
Edit LAG | 543 |
Edit LAG | 544 |
Edit LAG | 546 |
Edit LAG | 547 |
Edit LAG | 548 |
Edit LAG | 549 |
Edit LAG | 550 |
Add LAG | 200 |
Add LAG | 500 |
Add LAG | 502 |
Add LAG | 503 |
Add LAG | 504 |
Add LAG | 509 |
Add LAG | 510 |
Add LAG | 541 |
Add LAG | 542 |
Add LAG | 543 |
Add LAG | 544 |
Add LAG | 545 |
Add LAG | 546 |
Add LAG | 547 |
Add LAG | 548 |
Add LAG | 550 |

) Copyright 2017 Sophos Limited. All rights reserved.
Sophos is registered trademarks of Sophos Limited and Sophos Group. All other product and company names mentioned are trademarks or registered trademarks of their respective owners.No part of this publication may be reproduced, stored in a retrieval system, or transmitted, in any form or by any means, electronic, mechanical, photocopying, recording or otherwise unless you are either a valid licensee where the documentation can be reproduced in accordance with the license terms or you otherwise have the prior permission in writing of the copyright owner.