Operation: | Add DNS Host Entry / Edit DNS Host Entry
Description: | To Add/Edit DNS Host Entry which allows adding DNS mapping of domain with IPv4/IPv6 Address.Maximum 8 addresses are allowed in one DNS Host Entry.

Sample Configuration
    	<DNSHostEntry>
    		<HostName>hostname</HostName>
    		<AddressList><!-- only 8 addresses are supported -->
    			<Address>
    				<EntryType>Manual/InterfaceIP</EntryType>
    				<IPFamily>IPv4/IPv6</IPFamily>
    				<IPAddress>ip address</IPAddress><!-- When EntryType is InterfaceIP interface name is required. -->
    				<TTL>Number</TTL>
    				<Weight>Number</Weight>
    				<PublishOnWAN>Enable/Disable</PublishOnWAN>
    			</Address>
    			:
    			:
    			:
    		</AddressList>
    		<AddReverseDNSLookUp>Enable/Disable</AddReverseDNSLookUp>
    	</DNSHostEntry>

Attribute/Parameter Information :

Parameter | Mandatory | Default | Description
--- | --- | --- | ---
HostName | Yes |  | Description: Specify a Fully Qualified Domain Name(FQDN) for Host/Domain. HostName confines to: Type is 'SCALAR'. Datatype is 'FQDN'. Maximum characters allowed are 253.
IPFamily | Yes |  | Description: Select the type of family. IPFamily confines to: Type is 'ARRAY'. Datatype is 'STRING'. Only '1', '0' are allowed. Multiple values are allowed. Duplicate values will not be ignored.
EntryType | Yes |  | Description: Select Entry type from the available options: Manual or Interface IP. EntryType confines to: Type is 'ARRAY'. Datatype is 'STRING'. Only '1', '0' are allowed. Multiple values are allowed. Duplicate values will not be ignored.
IPAddress | Yes |  | Description: Select the IPv4/IPv6 address to be mapped to the domain. IPAddress confines to: Type is 'ARRAY'. Datatype is 'STRING'. Multiple values are allowed. Duplicate values will not be ignored.
TTL | Yes | 3600 | Description: Specify Time to Live in seconds. TTL confines to: Type is 'ARRAY'. Datatype is 'INTEGER'. Range 1 to 604800 is allowed. Maximum digits allowed are 6. Multiple values are allowed. Duplicate values will not be ignored.
Weight | Yes |  | Description: Specify weight for load balancing the traffic. Weight confines to: Type is 'ARRAY'. Datatype is 'INTEGER'. Range 0 to 255 is allowed. Maximum digits allowed are 3. Multiple values are allowed. Duplicate values will not be ignored.
PublishOnWAN | Yes |  | Description: Enable to publish DNS Host Entry on WAN. PublishOnWAN confines to: Type is 'ARRAY'. Datatype is 'INTEGER'. Only '1', '0' are allowed. Multiple values are allowed. Duplicate values will not be ignored.
AddReverseDNSLookUp | No | Disable | Description: Enable to allow reverse DNS lookup. AddReverseDNSLookUp confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only '1' are allowed.

Status Message Information :

Operation | Status | Message
--- | --- | ---
Edit DNS Host Entry | 200 |
Edit DNS Host Entry | 500 |
Edit DNS Host Entry | 502 |
Edit DNS Host Entry | 503 |
Add DNS Host Entry | 200 |
Add DNS Host Entry | 500 |
Add DNS Host Entry | 502 |
Add DNS Host Entry | 503 |
Add DNS Host Entry | 510 |
Add DNS Host Entry | 541 |

) Copyright 2017 Sophos Limited. All rights reserved.
Sophos is registered trademarks of Sophos Limited and Sophos Group. All other product and company names mentioned are trademarks or registered trademarks of their respective owners.No part of this publication may be reproduced, stored in a retrieval system, or transmitted, in any form or by any means, electronic, mechanical, photocopying, recording or otherwise unless you are either a valid licensee where the documentation can be reproduced in accordance with the license terms or you otherwise have the prior permission in writing of the copyright owner.