Operation: | Update Access Point
Description: | The page allows one to update Access Points.

Sample Configuration
    	<WirelessAccessPoint>
    		<ID>A40016ADB63B7F1</ID>
    		<Label>AP30[A40016ADB63B7F1]</Label>
    		<Country>India</Country>
    		<Group>No Group/wlgroup</Group>
    		<WirelessNetworks>
    			<Network>wlnet1</Network>
    			<Network>wlnet2</Network>
    		</WirelessNetworks>
    		<MeshNetwoks>
    			<MeshNetwok>
    				<MeshID>mesh1</MeshID>
    				<Role>RootAccessPoint</Role>
    			</MeshNetwok>
    			<MeshNetwok>
    				<MeshID>mesh2</MeshID>
    				<Role>RootAccessPoint</Role>
    			</MeshNetwok>
    		</MeshNetwoks>
    		<Channel2.4GHz>Auto/1/2/3</Channel2.4GHz>
    		<DynChan>Enable</DynChan>
    		<TimeBasedScan>Enable</TimeBasedScan>
    		<ScanTime>
    			<Time>All Time on Weekends</Time>
    		</ScanTime>
    		<TXPower>100%</TXPower>
    		<Channel5GHz>Auto/1/2/3</Channel5GHz>
    		<DynChan5GHz>Enable</DynChan5GHz>
    		<TimeBasedScan5GHz>Enable</TimeBasedScan5GHz>
    		<ScanTime5GHz>
    			<Time>All Time on Weekends</Time>
    		</ScanTime5GHz>
    		<TXPower5GHz>100%</TXPower5GHz>
    		<STP>Enable/Disable</STP>
    		<VLANTagging>Enable</VLANTagging>
    		<APVLANID>25</APVLANID>
    	</WirelessAccessPoint>

Attribute/Parameter Information :

Parameter | Mandatory | Default | Description
--- | --- | --- | ---
ID | Yes |  | Description: Displays ID of the Access Point. ID confines to: Type is 'SCALAR'. Datatype is 'STRING'.
Label | Yes |  | Description: Specify label Label confines to: Type is 'SCALAR'. Datatype is 'STRING'. Comma (,) is not allowed. Maximum characters allowed are 30. UTF-8 character(s) are allowed.
Country | Yes |  | Description: Select Country where the Access Point is located. Country confines to: Type is 'SCALAR'. Datatype is 'STRING'.
Group | No |  | Description: Select Access point group for the Access Point. Group confines to: Type is 'SCALAR'. Datatype is 'STRING'.
Network | No |  | Description: Select Wireless Networks for the Access Point. Network confines to: Type is 'ARRAY'. Datatype is 'STRING'. Multiple values are allowed. Duplicate values will not be ignored.
Role | No |  | Description: Select role for the Access Point. Role confines to: Type is 'ARRAY'. Datatype is 'STRING'. Only 'point', 'portal' are allowed. Multiple values are allowed. Duplicate values will not be ignored.
Channel2.4GHz | No |  | Description: Select a channel that will be used by the access point.(2.4 GHz) Channel2.4GHz confines to: Type is 'SCALAR'. Datatype is 'STRING'.
DynChan | No | Disable | Description: Select this to enable Access Point to scan for channels dynamically.(5 GHz) DynChan confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only 't' are allowed.
TimeBasedScan | No | Disable | Description: Select this to enable Time Based scan for Access Point.(2.4 GHz) TimeBasedScan confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only 't' are allowed. Note: Applicable only if Dyn Chan is enabled..
TXPower | No | 100% | Description: Select the transmission power for the Access Point. TXPower confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only '10', '25', '50', '75', '100' are allowed.
Channel5GHz | No |  | Description: Select a channel that will be used by the access point.(2.4 GHz) Channel5GHz confines to: Type is 'SCALAR'. Datatype is 'STRING'.
DynChan5GHz | No | Disable | Description: Select this to enable Access Point to scan for channels dynamically.(5 GHz) DynChan5GHz confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only 't' are allowed.
TimeBasedScan5GHz | No | Disable | Description: Select this to enable Time Based scan for Access Point.(5 GHz) TimeBasedScan5GHz confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only 't' are allowed. Note: Applicable only if Dyn Chan is enabled..
Time | No |  | Description: Select Scan Time for the Access Point(5 GHz). Time confines to: Type is 'ARRAY'. Datatype is 'STRING'. Multiple values are allowed. Note: Applicable only if 'Time Based scan'(5 GHz) is enabled..
TXPower5GHz | No | 100% | Description: Select the transmission power output for 5 GHz band. TXPower5GHz confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only '10', '25', '50', '75', '100' are allowed.
STP | No | Disable | Description: Select to use Spanning Tree protocol (STP). STP confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only '0', '1' are allowed.
VLANTagging | No | Disable | Description: Select this to enable VLAN tagging and to connect Access Point with an existing VLAN Ethernet Interface. VLANTagging confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only '0', '1' are allowed.
APVLANID | No | 2 | Description: Specify the VLAN ID that will be used by the AP to connect to the appliance. APVLANID confines to: Type is 'SCALAR'. Datatype is 'INTEGER'. Range 2 to 4094 is allowed. Maximum digits allowed are 4. Note: Available only when 'VLan Tagging' is selected..
Time | No |  | Description: Select Scan Time for the Access Point(2.4 GHz). Time confines to: Type is 'ARRAY'. Datatype is 'STRING'. Multiple values are allowed. Note: Applicable only if 'Time Based scan'(2.4 GHz) is enabled..
ACAbility | Yes |  | Description: Specify 'band' ACAbility confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only 'a', 'g' are allowed.
MeshID | No |  | Description: Select Mesh Networks for the Access Point. MeshID confines to: Type is 'ARRAY'. Datatype is 'STRING'. Multiple values are allowed. Duplicate values will not be ignored.

Status Message Information :

Operation | Status | Message
--- | --- | ---
Update Access Point | 200 |
Update Access Point | 500 |
Update Access Point | 523 |
Update Access Point | 524 |
Update Access Point | 542 |
Update Access Point | 216 |
Update Access Point | 541 |
Update Access Point | 543 |
Update Access Point | 545 |
Update Access Point | 544 |
Update Access Point | 547 |

) Copyright 2017 Sophos Limited. All rights reserved.
Sophos is registered trademarks of Sophos Limited and Sophos Group. All other product and company names mentioned are trademarks or registered trademarks of their respective owners.No part of this publication may be reproduced, stored in a retrieval system, or transmitted, in any form or by any means, electronic, mechanical, photocopying, recording or otherwise unless you are either a valid licensee where the documentation can be reproduced in accordance with the license terms or you otherwise have the prior permission in writing of the copyright owner.