Operation: | Add Multicast Route / Edit Multicast Route
Description: | To Add/Update Multicast Route. Multicast Route delivers the traffic generated from a single source to multiple receivers.

Sample Configuration
    	<MulticastRoute>
    		<SourceIPAddress>ipaddress</SourceIPAddress>
    		<SourceInterface>PortA</SourceInterface>
    		<SourceTunnel>SystemInterface/IPSec/GRE</SourceTunnel>
    		<MulticastAddress>ipaddress</MulticastAddress>
    		<DestinationInterfaceList>
    			<DestinationInterface>
    				<!-- For TunnelType IPSec give 'IPSec Connection' in 'Interface' tag -->
    				<Interface>PortB</Interface>
    				<TunnelType>SystemInterface/IPSec/GRE</TunnelType>
    			</DestinationInterface>
    			:
    		</DestinationInterfaceList>
    		<OldConfiguration>
    			<SourceIPAddress>ipaddress</SourceIPAddress>
    			<MulticastAddress>ipaddress</MulticastAddress>
    		</OldConfiguration>

    	</MulticastRoute>

Attribute/Parameter Information :

Parameter | Mandatory | Default | Description
--- | --- | --- | ---
SourceIPAddress | Yes |  | Description: Specify Source IPv4 address. SourceIPAddress confines to: Type is 'SCALAR'. Datatype is 'IPADDRESS'. IP Class other than 'MULTICAST', 'RESERVED', 'LOCALHOST', 'UNSPECIFIED', 'BROADCAST', 'LINKLOCAL' is allowed.
SourceTunnel | No |  | Description: Select Source Tunnel from the available options: System Interface, IPSec or GRE. SourceTunnel confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only 'systeminterface', 'ipsec', 'gre' are allowed.
SourceInterface | No |  | Description: Select Source Interface from the list. SourceInterface confines to: Type is 'SCALAR'. Datatype is 'STRING'.
MulticastAddress | Yes |  | Description: Specify the Multicast IPv4 Address. MulticastAddress confines to: Type is 'SCALAR'. Datatype is 'IPADDRESS'.
TunnelType | No |  | Description: Select Destination Tunnel Type from the available options: System Interface, IPSec or GRE. TunnelType confines to: Type is 'ARRAY'. Datatype is 'STRING'. Only 'systeminterface', 'ipsec', 'gre' are allowed. Multiple values are allowed.
Interface | No |  | Description: Select Destination Interface from the list. Interface confines to: Type is 'ARRAY'. Datatype is 'STRING'. Multiple values are allowed.

Status Message Information :

Operation | Status | Message
--- | --- | ---
Edit Multicast Route | 200 |
Edit Multicast Route | 211 |
Edit Multicast Route | 212 |
Edit Multicast Route | 213 |
Edit Multicast Route | 214 |
Edit Multicast Route | 500 |
Edit Multicast Route | 504 |
Edit Multicast Route | 547 |
Edit Multicast Route | 541 |
Edit Multicast Route | 542 |
Edit Multicast Route | 543 |
Edit Multicast Route | 544 |
Edit Multicast Route | 545 |
Edit Multicast Route | 546 |
Add Multicast Route | 200 |
Add Multicast Route | 211 |
Add Multicast Route | 212 |
Add Multicast Route | 213 |
Add Multicast Route | 214 |
Add Multicast Route | 500 |
Add Multicast Route | 504 |
Add Multicast Route | 547 |
Add Multicast Route | 541 |
Add Multicast Route | 542 |
Add Multicast Route | 543 |
Add Multicast Route | 544 |
Add Multicast Route | 545 |

) Copyright 2017 Sophos Limited. All rights reserved.
Sophos is registered trademarks of Sophos Limited and Sophos Group. All other product and company names mentioned are trademarks or registered trademarks of their respective owners.No part of this publication may be reproduced, stored in a retrieval system, or transmitted, in any form or by any means, electronic, mechanical, photocopying, recording or otherwise unless you are either a valid licensee where the documentation can be reproduced in accordance with the license terms or you otherwise have the prior permission in writing of the copyright owner.