Operation: | Add Failover Connection Group / Update Failover Connection Group.
Description: | To Create/Update Failover Connection Group which is a group of connections that are used for failover to provide continuous VPN connectivity for IPSEC connection.To update Failover group.

Sample Configuration
    	<VPNFailoverGroup>
    		<GroupDetail>
    			<Name>failovergroupname</Name>
    			<MemberConnections>
    				<Connection>connectionname</Connection>
    				:
    			</MemberConnections>
    			<MailNotification>Enable/Disable</MailNotification>
    			<FailoverCondition>
    				<FailoverIF>
    					<Protocol>PING/TCP</Protocol>
    					<Port>Number</Port>
    				</FailoverIF>
    				:
    			</FailoverCondition>
    		</GroupDetail>
    		<Active>
    			<Name>failovergroupname</Name>
    		</Active>
    		<DeActive>
    			<Name>failovergroupname</Name>
    		</DeActive>
    	</VPNFailoverGroup>

Attribute/Parameter Information :

Parameter | Mandatory | Default | Description
--- | --- | --- | ---
Name | Yes |  | Description: Specify a name for the Connection Group. Name confines to: Type is 'SCALAR'. Datatype is 'STRING'. First character is to be alphabet (a-zA-Z). Alphanumeric (a-zA-Z0-9) and underscore (_) to be allowed for the remaining characters.
Connection | Yes |  | Description: Select the Connection to be added to Member Connection List. Connection confines to: Type is 'ARRAY'. Datatype is 'STRING'. Multiple values are allowed.
MailNotification | No |  | Description: Enable Mail Notification to receive Connection failure notification. MailNotification confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only 'y', 'n' are allowed.
Protocol | No |  | Description: Specify Communication Protocol to configure VPN failover rules. Protocol confines to: Type is 'ARRAY'. Datatype is 'STRING'. Only 'ping', 'tcp', '' are allowed. Multiple values are allowed. Duplicate values will not be ignored.
Port | No |  | Description: Specify Port number for communication in case of TCP communication. Port confines to: Type is 'ARRAY'. Datatype is 'STRING'. Multiple values are allowed. Allowed numbers: 1 to 65535.

Status Message Information :

Operation | Status | Message
--- | --- | ---
Update Failover Connection Group. | 200 |
Update Failover Connection Group. | 500 |
Update Failover Connection Group. | 502 |
Add Failover Connection Group | 200 |
Add Failover Connection Group | 500 |
Add Failover Connection Group | 502 |

) Copyright 2017 Sophos Limited. All rights reserved.
Sophos is registered trademarks of Sophos Limited and Sophos Group. All other product and company names mentioned are trademarks or registered trademarks of their respective owners.No part of this publication may be reproduced, stored in a retrieval system, or transmitted, in any form or by any means, electronic, mechanical, photocopying, recording or otherwise unless you are either a valid licensee where the documentation can be reproduced in accordance with the license terms or you otherwise have the prior permission in writing of the copyright owner.