Operation: | Add Bridge-Pair / Edit Bridge-Pair
Description: | To Add/Update Bridge Pair configuration.

Sample Configuration
    	<BridgePair>
    		<Name>bridgepairname</Name>
    		<Description>Text</Description>
    		<RoutingOnBridgePair>Enable/Disable</RoutingOnBridgePair>
    		<BridgeMembers>
    			<Member>
    				<Interface>interfacename</Interface>
    				<Zone>zonename</Zone>
    			</Member>
    			<Member>
    				<Interface>interfacename</Interface>
    				<Zone>zonename</Zone>
    			</Member>
    			:
    		</BridgeMembers>
    		<!-- IPv4 configuration -->
    		<IPv4Configuration>Enable/Disable</IPv4Configuration>
    		<IPAddress>ip address</IPAddress>
    		<Netmask>netmask</Netmask>
    		<Gateway>
    			<GatewayName>Text</GatewayName>
    			<GatewayIPAddress>ip address</GatewayIPAddress>
    		</Gateway>

    		<!-- IPv6 configuration -->
    		<IPv6Configuration>Enable/Disable</IPv6Configuration>
    		<IPv6Address>ipv6 address</IPv6Address>
    		<Prefix>Number</Prefix>
    		<IPv6Gateway>
    			<IPv6GatewayName>Text</IPv6GatewayName>
    			<IPv6GatewayIPAddress>ipv6 address</IPv6GatewayIPAddress>
    		</IPv6Gateway>
    		<MTU>Number</MTU>
    		<MSS>
    			<Override>Enable/Disable</Override>
    			<MSSValue>Number</MSSValue>
    		</MSS>
    	</BridgePair>

Attribute/Parameter Information :

Parameter | Mandatory | Default | Description
--- | --- | --- | ---
Name | Yes |  | Description: Specify a name to identify the bridge-pair. Name confines to: Type is 'SCALAR'. Datatype is 'STRING'. First character is to be alphabet (a-zA-Z). Alphanumeric (a-zA-Z0-9) and underscore (_) to be allowed for the remaining characters. Maximum characters allowed are 10.
Description | No |  | Description: Specify description for the bridge-pair. Description confines to: Type is 'SCALAR'. Datatype is 'STRING'. Maximum characters allowed are 100.
RoutingOnBridgePair | No |  | Description: Used to enable routing on bridge-pair. RoutingOnBridgePair confines to: Type is 'SCALAR'. Datatype is 'STRING'.
IPv4Configuration, IPv6Configuration | Yes |  | Description: Used to determine whether the IP type is IPv4 or IPv6. IPv4Configuration,IPv6Configuration confines to: Type is 'ARRAY'. Datatype is 'STRING'. Maximum characters allowed are 2. Only '0', '1' are allowed. Multiple values are allowed.
Interface | Yes |  | Description: Used to select member interfaces in bridge-pair. Interface confines to: Type is 'ARRAY'. Datatype is 'STRING'. Maximum characters allowed are 15. Multiple values are allowed.
Zone | Yes |  | Description: Used to select Zones to which the interfaces belong in the bridge-pair. Zone confines to: Type is 'ARRAY'. Datatype is 'STRING'. Maximum characters allowed are 60. Multiple values are allowed. Duplicate values will not be ignored.
IPAddress | Yes |  | Description: Specify IPv4 Address for IPv4 Configuration. IPAddress confines to: Type is 'SCALAR'. Datatype is 'IPADDRESS'. Maximum characters allowed are 15. IP Class other than 'MULTICAST', 'RESERVED', 'LOCALHOST', 'UNSPECIFIED', 'BROADCAST', 'NETWORKBROADCAST', 'NETWORKIP' is allowed.
Netmask | Yes |  | Description: Specify Network Subnet mask for IPv4 Configuration. Netmask confines to: Type is 'SCALAR'. Datatype is 'IPADDRESS'. Maximum characters allowed are 15.
GatewayName | No |  | Description: Specify Gateway name for IPv4 Configuration. GatewayName confines to: Type is 'SCALAR'. Datatype is 'STRING'. Maximum characters allowed are 50.
GatewayIPAddress | No |  | Description: Specify Gateway IP Address for IPv4 Configuration. GatewayIPAddress confines to: Type is 'SCALAR'. Datatype is 'IPADDRESS'. Maximum characters allowed are 15. IP Class other than 'MULTICAST', 'RESERVED', 'LOCALHOST', 'UNSPECIFIED', 'BROADCAST', 'NETWORKBROADCAST', 'NETWORKIP' is allowed.
IPv6Address | No |  | Description: Specify IPv6 Address for IPv6 Configuration. IPv6Address confines to: Type is 'SCALAR'. Datatype is 'IPADDRESS6'. Maximum characters allowed are 45. IP Class other than 'MULTICAST', 'LOCALHOST', 'UNSPECIFIED', 'BROADCAST', 'LINKLOCAL', 'NETWORKBROADCAST', 'NETWORKIP' is allowed.
Prefix | Yes |  | Description: Specify Network Subnet mask Prefix for IPv6 Configuration. Prefix confines to: Type is 'SCALAR'. Datatype is 'INTEGER'. Range 1 to 128 is allowed. Maximum digits allowed are 40.
IPv6GatewayName | No |  | Description: Specify Gateway Name for IPv6 Configuration. IPv6GatewayName confines to: Type is 'SCALAR'. Datatype is 'STRING'. Maximum characters allowed are 50.
IPv6GatewayIPAddress | No |  | Description: Specify Gateway IP Address for IPv6 Configuration. IPv6GatewayIPAddress confines to: Type is 'SCALAR'. Datatype is 'IPADDRESS6'. Maximum characters allowed are 45. IP Class other than 'MULTICAST', 'LOCALHOST', 'UNSPECIFIED', 'BROADCAST', 'NETWORKBROADCAST', 'NETWORKIP' is allowed.
MTU | Yes | 1500 | Description: Used to set Maximum Transmission Unit value which is the largest physical packet size. MTU confines to: Type is 'SCALAR'. Datatype is 'INTEGER'. Range 1280 to 1500 is allowed.
Override | No |  | Description: Used to override existing MSS with new MSS. Override confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only 'on' are allowed.
MSSValue | Yes | 1460 | Description: Used to set Maximum Segment Size which is the amount of data that can be transmitted in a single packet. MSSValue confines to: Type is 'SCALAR'. Datatype is 'INTEGER'. Range 536 to 1460 is allowed.

Status Message Information :

Operation | Status | Message
--- | --- | ---
Edit Bridge-Pair | 200 |
Edit Bridge-Pair | 500 |
Edit Bridge-Pair | 503 |
Edit Bridge-Pair | 504 |
Edit Bridge-Pair | 508 |
Edit Bridge-Pair | 510 |
Edit Bridge-Pair | 541 |
Edit Bridge-Pair | 542 |
Edit Bridge-Pair | 543 |
Edit Bridge-Pair | 544 |
Edit Bridge-Pair | 545 |
Edit Bridge-Pair | 546 |
Add Bridge-Pair | 200 |
Add Bridge-Pair | 500 |
Add Bridge-Pair | 502 |
Add Bridge-Pair | 503 |
Add Bridge-Pair | 504 |
Add Bridge-Pair | 508 |
Add Bridge-Pair | 510 |
Add Bridge-Pair | 541 |
Add Bridge-Pair | 542 |
Add Bridge-Pair | 543 |
Add Bridge-Pair | 544 |

) Copyright 2017 Sophos Limited. All rights reserved.
Sophos is registered trademarks of Sophos Limited and Sophos Group. All other product and company names mentioned are trademarks or registered trademarks of their respective owners.No part of this publication may be reproduced, stored in a retrieval system, or transmitted, in any form or by any means, electronic, mechanical, photocopying, recording or otherwise unless you are either a valid licensee where the documentation can be reproduced in accordance with the license terms or you otherwise have the prior permission in writing of the copyright owner.