Operation: | Add Unicast Route / Update Unicast Route
Description: | To Add/Update Unicast Route. A Route provides the appliance with the information it needs to forward a packet to a particular destination.

Sample Configuration
    	<UnicastRoute>
    		<IPFamily>IPv4/IPv6</IPFamily>
    		<DestinationIP>ipaddress</DestinationIP>
    		<Netmask>0.0.0.0</Netmask>
    		<Gateway>ipaddress</Gateway>
    		<Interface>PortA</Interface>
    		<Distance>0</Distance>
    		<OldConfiguration>
    			<DestinationIP>ipaddress</DestinationIP>
    			<Netmask>0.0.0.0</Netmask>
    			<Gateway>ipaddress</Gateway>
    			<Interface>PortA</Interface>
    			<Distance>0</Distance>
    		</OldConfiguration>
    	</UnicastRoute>

Attribute/Parameter Information :

Parameter | Mandatory | Default | Description
--- | --- | --- | ---
DestinationIP | Yes |  | Description: Specify destination IPv4/IPv6 address. DestinationIP confines to: Type is 'SCALAR'. Datatype is 'IPADDRESS6'. Maximum characters allowed are 45. IP Class other than 'MULTICAST', 'LOCALHOST' is allowed.
Netmask | Yes |  | Description: Select Network Subnet mask prefix from the available options. Netmask confines to: Type is 'SCALAR'. Datatype is 'INTEGER'. Range 0 to 128 is allowed.
Gateway | No |  | Description: Specify Gateway IPv4 address. Gateway confines to: Type is 'SCALAR'. Datatype is 'IPADDRESS','IPADDRESS6'. Maximum characters allowed are 45. IP Class other than 'MULTICAST', 'RESERVED', 'LOCALHOST', 'UNSPECIFIED', 'BROADCAST', 'LINKLOCAL' is allowed.
Interface | No |  | Description: Select interface from the options available. Interface confines to: Type is 'SCALAR'. Datatype is 'STRING'.
Distance | No | 0 | Description: Specify distance for routing. Distance confines to: Type is 'SCALAR'. Datatype is 'INTEGER'. Range 0 to 255 is allowed. Maximum digits allowed are 3.
IPFamily | No | IPv4 | Description: Specify 'ipfamily' IPFamily confines to: Type is 'SCALAR'. Datatype is 'INTEGER'.

Status Message Information :

Operation | Status | Message
--- | --- | ---
Update Unicast Route | 200 |
Update Unicast Route | 500 |
Update Unicast Route | 502 |
Update Unicast Route | 541 |
Update Unicast Route | 510 |
Update Unicast Route | 511 |
Update Unicast Route | 526 |
Add Unicast Route | 200 |
Add Unicast Route | 500 |
Add Unicast Route | 502 |
Add Unicast Route | 541 |
Add Unicast Route | 510 |
Add Unicast Route | 511 |

) Copyright 2015 Sophos Limited. All rights reserved.
Sophos is registered trademarks of Sophos Limited and Sophos Group. All other product and company names mentioned are trademarks or registered trademarks of their respective owners.No part of this publication may be reproduced, stored in a retrieval system, or transmitted, in any form or by any means, electronic, mechanical, photocopying, recording or otherwise unless you are either a valid licensee where the documentation can be reproduced in accordance with the license terms or you otherwise have the prior permission in writing of the copyright owner.