Operation: | Add Wireless Network / Update Wireless Network
Description: | Add Wireless Network and Update Wireless Network

Sample Configuration
    	<WirelessNetworks>
    		<Name>wlnet1</Name>
    		<SSID>wlnet123</SSID>
    		<SecurityMode>WPA2Personal</SecurityMode>
    		<Key>123456789</Key>
    		<ClientTraffic>SeparateZone</ClientTraffic>
    		<Zone>LAN</Zone>
    		<IPAddress>12.12.12.12</IPAddress>
    		<Netmask>255.255.255.0</Netmask>
    		<BridgetoVLANid>15</BridgetoVLANid>
    		<Description>test wlnet</Description>
    		<Encryption>TKIP(only abg)</Encryption>
    		<FrequencyBand>2.4and5GHz</FrequencyBand>
    		<ClientIsolation>Enable</ClientIsolation>
    		<HideSSID>Enable</HideSSID>
    	</WirelessNetworks>

Attribute/Parameter Information :

Parameter | Mandatory | Default | Description
--- | --- | --- | ---
Name | Yes |  | Description: Enter a descriptive name for the network. Name confines to: Type is 'SCALAR'. Datatype is 'STRING'.
Description | No |  | Description: Enter a description for the wireless network that helps you to identify it. Description confines to: Type is 'SCALAR'. Datatype is 'STRING'.
SSID | Yes |  | Description: Enter the Service Set Identifier (SSID) for the network to identify the wireless network. SSID confines to: Type is 'SCALAR'. Datatype is 'STRING'.
SecurityMode | Yes | WPA2 Personal | Description: Select a security mode. SecurityMode confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only '0', '3', '4', '5', '6', '7', '8', '9' are allowed.
Key | No |  | Description: Enter the passphrase to protect the wireless network from unauthorized access. Key confines to: Type is 'SCALAR'. Datatype is 'STRING'. Note: Applicable only if Security Mode is selected as 'WPA Personal', 'WPA2Personal' or 'WPA2/WPA Personal'..
ClientTraffic | Yes | Separate Zone | Description: Select a method to integrate wireless network into local network. ClientTraffic confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only 'none', 'lan', 'vlan' are allowed.
Zone | No |  | Description: Specify Zone Zone confines to: Type is 'SCALAR'. Datatype is 'STRING'.
Client VLAN ID | No |  | Description: Specify Client VLAN ID Client VLAN ID confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only '0', '1' are allowed.
Encryption | No | TKIP (only abg) | Description: Select an encryption algorithm. Encryption confines to: Type is 'SCALAR'. Datatype is 'STRING'. Note: Not Applicable if Security Mode is selected as 'No Encryption' or 'WEP Open'..
TimeBasedAccess | No | Disable | Description: Enable or Disable the wireless network according to a time schedule. TimeBasedAccess confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only '1', '0' are allowed.
Time | No |  | Description: Select a schedule definition which determines when the wireless network is enabled. Time confines to: Type is 'ARRAY'. Datatype is 'STRING'. Multiple values are allowed. Note: Applicable only if 'Time-based Access' is Enabled..
ClientIsolation | Yes | Disabled | Description: Enable or disable to deny or allow clients within a network to communicate with one another. ClientIsolation confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only '0', '1' are allowed.
HideSSID | No | Disable | Description: Enable or disable to hide or display wireless network's SSID. HideSSID confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only '0', '1' are allowed.
FastTransition | No |  | Description: Specify Enable or Disable FastTransition confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only '0', '1' are allowed.
MACFiltering | Yes | None | Description: Select the required approach to filter the MAC addresses that can be connected to this wireless network. MACFiltering confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only 'disable', 'allow', 'deny' are allowed.
MACList | No |  | Description: With Blacklist, all MAC addresses are allowed except those listed on the MAC List. With Whitelist, all MAC addresses are prohibited except those listed on the MAC List. MACList confines to: Type is 'SCALAR'. Datatype is 'STRING'. Note: Applicable only when MAC Filtering is selected as 'Whitelist' or 'Blacklist'..
BridgetoVLANid | No |  | Description: Enter the VLAN ID of the network that the wireless clients should be part of. BridgetoVLANid confines to: Type is 'SCALAR'. Datatype is 'INTEGER'. Range 0 to 4095 is allowed. Note: Applicable only if Client Traffic is selected as 'Bridge to VLAN'..
Netmask | No | /24(255.255.255.0) | Description: Select a subnet mask for the IP address. Netmask confines to: Type is 'SCALAR'. Datatype is 'STRING'. Note: Applicable only if Client Traffic is selected as 'Separate Zone'..
IPAddress | No |  | Description: Assign an IP address to the wireless network. IPAddress confines to: Type is 'SCALAR'. Datatype is 'STRING'. Note: Applicable only if Client Traffic is selected as 'Separate Zone'..
FrequencyBand | Yes | 2.4 and 5 GHz | Description: Select the frequency band at which the assigned access points of the wireless network should transmit. FrequencyBand confines to: Type is 'SCALAR'. Datatype is 'STRING'. Only 'a', 'g', 'ag' are allowed.
Key | No |  | Description: Enter a WEP key. Key confines to: Type is 'SCALAR'. Datatype is 'STRING'. Note: Applicable only if Security Mode is selected as 'WEP Open'..

Status Message Information :

Operation | Status | Message
--- | --- | ---
Update Wireless Network | 200 |
Update Wireless Network | 500 |
Update Wireless Network | 503 |
Update Wireless Network | 541 |
Update Wireless Network | 542 |
Update Wireless Network | 543 |
Update Wireless Network | 544 |
Update Wireless Network | 545 |
Update Wireless Network | 546 |
Update Wireless Network | 547 |
Add Wireless Network | 200 |
Add Wireless Network | 500 |
Add Wireless Network | 502 |
Add Wireless Network | 503 |
Add Wireless Network | 541 |
Add Wireless Network | 542 |
Add Wireless Network | 544 |
Add Wireless Network | 545 |

) Copyright 2017 Sophos Limited. All rights reserved.
Sophos is registered trademarks of Sophos Limited and Sophos Group. All other product and company names mentioned are trademarks or registered trademarks of their respective owners.No part of this publication may be reproduced, stored in a retrieval system, or transmitted, in any form or by any means, electronic, mechanical, photocopying, recording or otherwise unless you are either a valid licensee where the documentation can be reproduced in accordance with the license terms or you otherwise have the prior permission in writing of the copyright owner.